The resistance of the coil is 37.7 ohms.

After applying 5V to the coil, the current measured was 130 mA.